TEST CERTIFICATE
photo-sensitive epilepsy (PSE) flashing

This document certifies that the above programme/media was tested in full compliance 
with the requirements stated in:
RECOMMENDATION  ITU-R BT.1702-1 2018 Guidance for the reduction of photosensitive epileptic seizures caused by television (revised) as from 1st January 2019

Cel-Soft site number :	626238101

Installed at :			Facility Name
20 Facility Place
				London, W1T 1XYZ

Date:				26/11/2018
Time:				10:27:22
Title:				#title
Version:			V3.6 PSE V2.0  compliant to ITU-R BT.1702-1 2018
Tape/Media ID:		c:\users\robin palmer\documents\half flash test with 10s preroll x2 +tc.mxf
Picture Format:		1920 x 1080 fps:25.00

Duration			00:00:25:24  (Frames: 649)

PSE Test Result:		FAILED

SUMMARY OF TESTS:
Type of PSE Test Violation	Total frames	Events	
Red Flashes 	0	0	
 (Ofcom notes para 3)			
Spatial Pattarns 	0	0	
 (Ofcom notes para 5.1)			
Luma Flashes 	46	2	
 (Ofcom notes para 3)			
Extended flashes > 5secs	0	0	
 (Ofcom notes para 2)			

Checked by:			#operator                  Certificate version:		v3.5
cont..

Summary of test results 	Page 2  
Log:

PSE-Check log 26/11/2018 10:27:22 
Software versions: RCcontrolx 3.6.1 RC filter V3.6PSE:2.0 ITU-R BT.1702-1 2018 
log location= C:\Cel-Soft Results\half flash test with 10s preroll x2 +tc-9.rtf 
media -     > c:\users\robin palmer\documents\half flash test with 10s preroll x2 +tc.mxf 	
 	 Enabled Video Logging	
 PSE Flashes ON	 enabled 	
       PSE Luma Flashes	 enabled  fail threshold=25%	
       PSE Red Flashes	 enabled  fail threshold=25%	
       PSE Spatial Patterns	 enabled  fail threshold=47.3%	
       PSE Extended Flash	 enabled  fail threshold=18%	
 	Rec.709 matrix (HD) 	
 	
  --- PSE TEST SETTINGS AND VIOLATION EVENTS ---  	
 Test Duration=00:00:25:24  (Frames: 649) frame rate= 25	

  
 
 PSE ANALYSIS CHECKS 	
 PSE Luma Flashes	
    Test Results	  total events  =	  2	
 	  Total all error frames count =	  46	
 	  Total all errors duration =	  00:00:01:21	
 Overall	  Percentage of content with errors =	  7.1% of tested duration	
 	  No Percentage of content limit set 	  Not applicable	

 OVERALL PSE TEST RESULTS 	  FAILED on one parameter	
      Warnings 	  None	

 Test Results for PSE Checks:  FAILED	

 
 
 --- PSE FLASH TESTS SUMMARY REPORT ---	
 	
 FAILED  	   Some PSE Checks had violations ! 	  Total (violations) fail events  = 2	
 	
 FAILED 	  PSE Luma flash 	  events detected = 2	
  	  PSE Luma flash 	  total frame counts = 46	
 PASSED 	  PSE  Red flash	  events detected = 0	
  	  PSE  Red flash	  total frame counts = 0	
 PASSED 	  PSE  Spatial pattern 	  events detected = 0	
  	  PSE  Spatial pattern 	  total frame counts = 0	
 	
 PSE Warnings	
 	
  	no warnings 	
 ==== end certificate document =====