#Logstart:

Media Logging Report Form 
(to build your own version of this template with your logo and text use Microsoft Word or whatever, and save in the 
C:\program files\celsoft\ReelChecksolo folder  as a  richtext file named: "Reel-Check Logfile template.rtf")

Project		Director		
Media		Colourist		
Reel		Editor		
Camera		Take		

Log:

PSE-Check log 26/11/2018 10:27:01 
Software versions: RCcontrolx 3.6.1 RC filter V3.6PSE:2.0 ITU-R BT.1702-1 2018 
log location= C:\Cel-Soft Results\half flash test with 10s preroll x2 +tc-9.rtf 
media -     > c:\users\cel-soft\documents\half flash test with 10s preroll x2 +tc.mxf 	

 
                               
                               VIDEO TESTS SETTINGS 	 All set parameters ON 	
 PSE Flashes ON	 enabled 	
       PSE Luma Flashes	 enabled  fail threshold=25%	
       PSE Red Flashes	 enabled  fail threshold=25%	
       PSE Spatial Patterns	 enabled  fail threshold=47.3%	
       PSE Extended Flash	 enabled  fail threshold=18%	
 Matrix Set	Rec.709 (HD) 	
 	
 Audio Logging 	 OFF  - Audio is present	

ü

>>> 10:00:00:03	:OK	log start	[TOD= 10:27:02] 	
	
10:00:11:02	:IN	PSE Luma Flashes = 74% 	 FAILED	
	
10:00:11:20	:OUT	PSE Luma Flashes violation cleared 23 frames		

10:00:19:05	:IN	PSE Luma Flashes = 74% 	 FAILED	
	
10:00:19:24	:OUT	PSE Luma Flashes violation cleared 23 frames		

	
10:00:26:00		Stopped logging	[TOD= 10:27:21] 	

finished data collection 	
Test Duration=00:00:25:24  (Frames: 649) frame rate= 25	
	
10:00:26:00	:OK	Media format found 		
1920 x 1080 fps:25.00 	

<<<

--- SUMMARY REPORT ---	

Test Duration=00:00:25:24  (Frames: 649) frame rate= 25	

VIDEO ANALYSIS TESTS 	
ALL VIDEO TESTS 	  PSE tested, no other video tests enabled 	

PSE ANALYSIS CHECKS 	
PSE Luma Flashes	
   Test Results	  total events  =	  2	
	  Total all error frames count =	  46	
	  Total all errors duration =	  00:00:01:21	
Overall	  Percentage of content with errors =	  7.1% of tested duration	
	  No Percentage of content limit set 	  Not applicable	

OVERALL PSE TEST RESULTS 	  FAILED on one parameter	
     Warnings 	  None	

	

--- PSE FLASH TESTS SUMMARY REPORT ---	
	
FAILED  	   Some PSE Checks had violations ! 	  Total (violations) fail events  = 2	
	
FAILED 	  PSE Luma flash 	  events detected = 2	
 	  PSE Luma flash 	  total frame counts = 46	
PASSED 	  PSE  Red flash	  events detected = 0	
 	  PSE  Red flash	  total frame counts = 0	
PASSED 	  PSE  Spatial pattern 	  events detected = 0	
 	  PSE  Spatial pattern 	  total frame counts = 0	
	
PSE Warnings	
	
 	no warnings